**Equipment Test of Selected Contractor**

The contracting authority shall request the selected contractor to meet as the condition for the conclusion of the contract a successful results of tests of samples in accordance with Section 104(1)(b) of the Act, i.e. a test of the offered equipment or the equipment which is similar to the equipment which is required by the Contracting authority to be delivered.

The required equipment test may be performed at the producer of the equipment or another client designate by the selected contractor.

In case the offered equipment is used or demonstration equipment, the selected contractor shall be obliged to perform the equipment test at the equipment which shall be delivered and not at similar equipment.

The contracting authority shall send the selected contractor its own data in 1bit TIFF format with resolution 10160 dpi on a DVD-ROM drive to perform the equipment test in order to generate the required printing plates and films. Other test material (printing plates and films) shall be provided by the contractor at his own costs.

The contracting authority shall require as the result of this test to create and return back to the contracting authority, within at least the 5 (words: five) working days of the receipt of the DVD-ROM drive with the data of the contracting Authority, the following:

1. two pieces of printing plates (see the specification below)
2. one piece of film (see the specification below)
3. DVD-ROM drive of the contracting authority.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Printing plate | 1060 x 795-820 | AL plates | 0,30 | BACHER 2000 |
| Printing plate | 1060 x 795-820 | NYLOPRINT | 0,73 | BACHER 2000 |
| Film | 1060 x 820 | diapositive |

The precise time limit for delivering the results of the test shall be given in the request of the contracting authority in accordance with the Section 122(3) of the Act.

The contracting authority shall verify the condition of the printing plates and film in accordance with the required tender conditions and mainly from the point of view of quality of creating individual component of motive (lines, rasters, etc.) within the keeping of the required resolution 10160 dpi and dimensional stability of exposure.

In case of finding out deficiencies or deviations by the verification of quality of delivered printing plates and film, the contracting authority shall exclude the selected contractor.

The same test shall be performed after installation and commissioning of the equipment at the contracting authority place.