**TECHNICAL SPECIFICATION BEYOND THE FRAMEWORK OF EUROPEAN LEGISLATION**

1. Sheet format 500 x 460 mm ± 1 mm (wide path)
2. The back of the paper (silicone paper) shall be provided with a visible print, which serves to prevent sheet rotation during paper processing at the client.