**TESTING PROCESS OF SAMPLES SUPPLIED BY THE TENDER WINNER**

The selected supplier will prove the fulfillment of the tender conditions by delivering 2000 sheets of self-adhesive paper for EU visa stickers with size 500 x 460 mm ± 1 mm (short grain), compliance of the required paper parameters with technical specifications and trouble-free printability on printing machines.

1. Test

**LABORATORY TEST**

Test progress:

For 10 sheets randomly selected from the delivered quantity of 2000 sheets, selected parameters will be measured in the contracting authority's laboratory and their conformity will be compared with the values ​​specified in the technical specification according to Commission Implementing Decision C (2018) 674 of 12 February 2018 and Regulation of the European Parliament and the European Council. 2017/1370.

2. Test

**PRINTING TEST ON PRODUCTION PRINTING MACHINES**

Test progress:

1990 sheets will be printed on the client's production printing machines using all printing techniques used in the production process of EU visa stickers. During printing, the smooth passage through the printing machines will be assessed, e.g. contamination of the machine with loose glue, adhesion of the Kinegram, formation of folds, cohesiveness of self-adhesive paper, drying of printing inks, etc.