**SAMPLE TESTING:**

**TESTING PROCESS OF A SAMPLE SUPPLIED BY THE SELECTED SUPPLIER**

The selected supplier shall prove the fulfilment of the tender conditions by delivering 1 roll of the printing paper to produce banknote binding tapes with width 180 mm and roll diameter 600 mm, compliance of the required paper parameters with technical specification (Annex No. 1 to the Draft Contract) and trouble-free processing on the flexo printing machines in the contracting authority premises.

**LABORATORY TEST**

Physical properties shall be measured in the contracting authority's laboratory and their conformity shall be compared with the values ​​specified in the technical specification (Annex No. 1 to the Draft Contract).

**PRINTING TEST ON PRODUCTION PRINTING MACHINES**

1 roll of the printing paper to produce banknote binding tapes shall be printed on the client's production printing machines. During printing, the printability, and the smooth passage of the paper through the printing machines, cutting into individual banknote binding tapes and gluing them with dextrin glue shall be assessed.