Packaging and storage conditions

1. Packaging

* The modules must be winded on the reel
* The defective modules in the reel must be marked by punched hole
* Each **reel must be labeled** and wrapped into an individual antistatic bag,
* Each bag must be packed in the cardboard box („pizza box“), that is also labeled and sealed
* „Pizza boxes“ should be stored in another cardboard box also labeled
* Arrangement of pizza boxes in cardboard box and arrangement of cardsboxes in the shipment will be specified by the Seller
* Labels should involve at least:
  + Product description
  + Product number
  + Batch number
  + Total number of modules in the reel, package
  + Number of failed modules
  + Date of production/expedition

2. Storage conditions

* Buyer’s standart storage conditions:

Temperature range 10 to 25°C with a maximum relative humidity of 60%

* The Seller may specify special storage conditions if it is necessary

3. Standard conditions of use

* Will be specified by the Seller