SAT Testing of the Numbering boxes

**SAT TESTS OF NEW NUMBERING BOXES FOR NUMEROTA II**

The Client will evaluate the level of adequate quality and stability of numbering application, ease of installation and replacement of numbering boxes (horizontal and vertical) while maintaining precise position in accordance with the requirements of the technical specification (hereinafter referred to as the “Device”).

1. **Tested material:**

2000 sheets will be numbered horizontally and vertically as part of the tests;

printed material in the range of 80 g/m2 - 90 g/m2

paper formats in the range of 590x570 - 710x530 mm

printed material - supplied by STC

1. **Acceptance / Check of the condition, quality, number of additional materials ordered with the delivery of the machine**

˗ new cams

- new holding rings

- new counterweights and center rings

- base parts of numbering boxes

- wheels assembly parts

˗ additional letter wheels

˗ additional number wheels

- functionality of setting gauge for inking rollers