**CTP transport way description**

1. The truck will drive and park in front of our STC premises (address: Růžová 6/943, 11000 Praha 1)
2. Machine and relating pallets will be unloaded from the truck by STC forklift (lifting capacity max.2,5 tons, higher lifting capacity on demand)
3. Machine and relating pallets will be moved by STC forklift to the premises. There is a space for unpacking and removing the pallets from the machine.
4. Afterwards the machines will be moved to the ramp and inside the lift

Lift dimensions:

width: 1340 mm

height: 2200 mm

depth: 2800 mm

loading capacity: 2800 kg

1. From the lift, we continue directly to the place of installation through the safe´s door (the door is the narrowest and crictical place on the transport way)

Safe´s door dimensions:

width: 1320 mm

height: 2100 mm

1. Then we follow to the place of installation – room No. 339 and relating drawing

**Maximum dimension of the machine or pallet must not exceed following sizes:**

**Width: 1300 mm**

**Lenght: 2800 mm**

**Height: 1900 mm**

You can see some pictures of the lift and safe´s door enclosed