Packaging and storage conditions

1. Packaging

* The modules must be winded on the reel
* The defective modules in the reel must be marked by punched hole
* Each **reel must be labeled** and wrapped into an individual antistatic bag,
* Each bag must be packed in the cardboard box („pizza box“), that is also labeled and sealed
* „Pizza boxes“ should be stored in another cardboard box also labeled
* Arrangement of pizza boxes in cardboard box and arrangement of cardsboxes in the shipment

will be specified by the Seller

* Labels should involve at least:

Product description

Product number

Batch number

Total number of modules in the reel, package

Number of failed modules + number of good modules

Date of production/expedition

2. Storage conditions

* Buyer’s standart storage conditions:

Temperature range 10 to 25°C with a maximum relative humidity of 60%

[the Contractor may complete with the data - may specify special storage conditions if it is necessary]

3. Standard conditions of use

[the Contractor shall complete with the data]